PCIM Change Proposal Status

|  |  |  |  |
| --- | --- | --- | --- |
| ID | Description | Author | Status |
| CP-PCD-##1 | * Terms for Universal Service Identifier * Association/Dissociation events * Begin/End Time Stamp clarifications | Eldon M |  |
| CP-PCD-##2 | * Single device per report | Eldon M |  |
| CP-PCD-##3 | * Deterministic Snapshot and Real-Time Results | Eldon M |  |
| CP-PCD-##4 | * DPAM->DPAR Error Responses | Bill H |  |
| CP-PCD-##5 | * Optional Order ID in PCD-17 | Tom K |  |
| CP-PCD-##? | * PCD-17 for all reports (can we re-use PCD-18) |  |  |
| CP-PCD-##? | * A.2.3.1 MSH uses IHE\_PCD\_017 and OID of .19 in MSH-21… Stick with forwarding of PCD-017 in structure and OID? |  |  |
| CP-PCD-##? | * PCD-19 for Snapshot and Real-time query and response |  |  |
| CP-PCD-##? | * PCD-## for Cancel (was also referenced as PCD-19, type and structure are different). |  |  |
| CP-PCD-##? | * Clarification of ACK types and required interactions for consumer and reporter to DPAM, update and clarify examples |  |  |
| CP-PCD-##? | * DPAC->DPAM error responses and associated use cases * Might be due to sync issues * DPAC could report corrected association status to manager… |  |  |
| CP-PCD-##? | * PCD-20 MFN\_M13 vs MFN\_M14 * PCD-20 MFE-3 for effective date/time, not MFE-7 * MFE.5 set to CWE, but MFE.4 is HD… Clarify. * Inconsistent use of CWE for PD for MFI.1. Spec states CWE, but valued INV. PCD uses RE, R and RE for first 3 of CWE. * PCD-20 Allow OBX segments to optionally carry model/manufacturer/serial as we do in other areas of PCD such as DEC and MEMDMC |  |  |
| CP-PCD-##? | * Combined reporter/manager role (testing only, or spec impacts) * Combined registrant/manager role (testing only or spec imapacts) |  |  |