IHE Change Proposal

Tracking information:

|  |  |
| --- | --- |
| IHE Domain | Patient Care Device (PCD) |
| Change Proposal ID: | CP-PCD-##2 |
| Change Proposal Status: | Draft |
| Date of last update: | 2022-05-24 |
| Person assigned: | Eldon Metz |

Change Proposal Summary information:

|  |  |
| --- | --- |
| PCIM Single Device Per Association/Disassociation Report Clarification | |
| Submitter’s Name(s) and e-mail address(es): | Eldon Metz, emetz@innovisionmedical.com |
| Submission Date: | TBD |
| Integration Profile(s) affected: | Point-of-Care Identity Management (PCIM) |
| Actor(s) affected: | Device-Patient Association Consumer  Device-Patient Association Manager  Device-Patient Association Reporter |
| IHE Technical Framework or Supplement modified: | PCIM Profile TI revision 1.1, dated 2018-12-07 |
| Volume(s) and Section(s) affected: | Trial Implementation, Multiple Sections |
| Rationale for Change:  Clarifications in the reporter introduction that a patient device reporter reports on a single device per report message.  This Change Proposal (CP) proposes changes to implement profile clarifications and positions for the above issues. | |
|  | |

Section **7.1.1.1 Device-Patient Association Reporter**, replace the paragraph on line 270 on page 14 to explicitly clarify a report is for a single device patient association event:

Existing Text:

The Device-Patient Association Reporter represents a system or person that is asserts that a given device is attached or removed from a specific patient. For each such event, the unique Patient ID, Device ID, and timestamp must be reported.

Proposed Text:

The Device-Patient Association Reporter represents a system or person that asserts in the form of a report that a specific device is attached or removed from a specific patient at an optionally specified location. Each report message represents a single device patient association assertion. For each such assertion event, the unique Patient ID, Device ID, and timestamp must be reported.